Because there’re so many case, so that I didn’t screen shot all

This VI is used for reading and writing data and error of data on connection and save it.

Mode : open, write, read, close

Question : I have answered in sab\_PLCloop.